Decoder related CTLs(3)

NAME
Decoder related CTLs -

  Defines
#define OPUS_SET_GAIN(x)
Configures decoder gain adjustment.
#define OPUS_GET_GAIN(x)
Gets the decoder's configured gain adjustment.

Detailed Description

See also:
    Generic CTLs, Encoder related CTLs, Opus Decoder

Define Documentation

  #define OPUS_GET_GAIN(x)

Gets the decoder's configured gain adjustment. See also:
    OPUS_SET_GAIN

Parameters:
    x opus_int32 *: Amount to scale PCM signal by in Q8 dB units.

  #define OPUS_SET_GAIN(x)

Configures decoder gain adjustment. Scales the decoded output by a factor specified in Q8 dB units. This has a maximum range of -32768 to 32767 inclusive, and returns OPUS_BAD_ARG otherwise. The default is zero indicating no adjustment. This setting survives decoder reset.

gain = pow(10, x/(20.0*256))

Parameters:
    x opus_int32: Amount to scale PCM signal by in Q8 dB units.

Author

Generated automatically by Doxygen for Opus from the source code.